###############################################################################
#                                                                             #
# IAR ELF Linker V5.41.0.51741/W32 for ARM              13/Dec/2013  19:08:42 #
# Copyright (C) 2007-2009 IAR Systems AB.                                     #
#                                                                             #
#    Output file  =  E:\WIZnet 产品文档\W5500\W5500\Application               #
#                    Reference\weibo_article\weibo\Debug\Exe\app.out          #
#    Map file     =  E:\WIZnet 产品文档\W5500\W5500\Application               #
#                    Reference\weibo_article\weibo\Debug\List\app.map         #
#    Command line =  "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\SPI2.o"          #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\core_cm3.o"      #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\device.o"        #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\main.o"          #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\mcu_init.o"      #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\md5.o"           #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\misc.o"          #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\socket.o"        #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\startup_stm32f10 #
#                    x_hd.o" "E:\WIZnet 产品文档\W5500\W5500\Application      #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_bkp.o" #
#                     "E:\WIZnet 产品文档\W5500\W5500\Application             #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_flash. #
#                    o" "E:\WIZnet 产品文档\W5500\W5500\Application           #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_gpio.o #
#                    " "E:\WIZnet 产品文档\W5500\W5500\Application            #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_it.o"  #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_rcc.o" #
#                     "E:\WIZnet 产品文档\W5500\W5500\Application             #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_spi.o" #
#                     "E:\WIZnet 产品文档\W5500\W5500\Application             #
#                    Reference\weibo_article\weibo\Debug\Obj\stm32f10x_usart. #
#                    o" "E:\WIZnet 产品文档\W5500\W5500\Application           #
#                    Reference\weibo_article\weibo\Debug\Obj\system_stm32f10x #
#                    .o" "E:\WIZnet 产品文档\W5500\W5500\Application          #
#                    Reference\weibo_article\weibo\Debug\Obj\util.o"          #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\w5500.o"         #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Obj\weibo.o" -o      #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\Exe\app.out" --map   #
#                    "E:\WIZnet 产品文档\W5500\W5500\Application              #
#                    Reference\weibo_article\weibo\Debug\List\app.map"        #
#                    --config "E:\WIZnet 产品文档\W5500\W5500\Application     #
#                    Reference\weibo_article\weibo\app.icf" --semihosting     #
#                    --entry __iar_program_start                              #
#                                                                             #
#                                                                             #
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

__endian      = little
__thumb_aware = enabled


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A1":  place at 0x08000000 { ro section .intvec };
"P1":  place in [from 0x08000000 to 0x0800ffff] { ro };
"P2":  place in [from 0x20000000 to 0x20004fff] {
          rw, block CSTACK, block HEAP };

  Section            Kind        Address    Size  Object
  -------            ----        -------    ----  ------
"A1":                                      0x130
  .intvec            ro code  0x08000000   0x130  startup_stm32f10x_hd.o [1]
                            - 0x08000130   0x130

"P1":                                     0x3628
  .text              ro code  0x08000130   0xcc2  xprintffull.o [3]
  .text              ro code  0x08000df4   0x580  w5500.o [1]
  .text              ro code  0x08001374   0x38c  socket.o [1]
  .text              ro code  0x08001700   0x340  stm32f10x_rcc.o [1]
  .text              ro code  0x08001a40   0x246  DblDiv.o [4]
  .text              ro code  0x08001c88   0x1b8  mcu_init.o [1]
  .text              ro code  0x08001e40   0x1a2  DblMul.o [4]
  .text              ro code  0x08001fe4   0x18a  stm32f10x_usart.o [1]
  .text              ro code  0x08002170   0x17e  DblSub.o [4]
  .text              ro code  0x080022f0   0x15c  stm32f10x_gpio.o [1]
  .text              ro code  0x0800244c   0x158  system_stm32f10x.o [1]
  .text              ro code  0x080025a4   0x150  device.o [1]
  .text              ro code  0x080026f4   0x130  weibo.o [1]
  .text              ro code  0x08002824   0x12e  I64DivMod.o [4]
  .text              ro code  0x08002954   0x108  xdscale.o [3]
  .text              ro code  0x08002a5c    0xe6  DblAdd.o [4]
  .text              ro code  0x08002b42    0xc6  xdnorm.o [3]
  .text              ro code  0x08002c08    0xb4  SPI2.o [1]
  .text              ro code  0x08002cbc    0xa0  misc.o [1]
  .rodata            const    0x08002d5c    0x9c  weibo.o [1]
  .text              ro code  0x08002df8    0x7c  stm32f10x_spi.o [1]
  .text              ro code  0x08002e74    0x7c  util.o [1]
  .text              ro code  0x08002ef0    0x70  ABImemcpy.o [4]
  .text              ro code  0x08002f60    0x66  ABImemset.o [4]
  .text              ro code  0x08002fc8    0x58  memchr.o [4]
  .text              ro code  0x08003020    0x56  DblToI32.o [4]
  .text              ro code  0x08003078    0x48  main.o [1]
  .text              ro code  0x080030c0    0x3c  stm32f10x_flash.o [1]
  .text              ro code  0x080030fc    0x38  ABImemset48.o [4]
  .text              ro code  0x08003134    0x36  strlen.o [4]
  .text              ro code  0x0800316c    0x30  sprintf.o [3]
  .text              ro code  0x0800319c    0x30  strstr.o [3]
  .text              ro code  0x080031cc    0x2e  DblCmpLe.o [4]
  .text              ro code  0x080031fc    0x2e  DblCmpGe.o [4]
  .text              ro code  0x0800322c    0x2e  I32ToDbl.o [4]
  .rodata            const    0x0800325c    0x24  main.o [1]
  .rodata            const    0x08003280    0x24  weibo.o [1]
  .text              ro code  0x080032a4    0x24  copy_init2.o [4]
  .iar.init_table    const    0x080032c8    0x24  - Linker created -
  .rodata            const    0x080032ec    0x20  main.o [1]
  .rodata            const    0x0800330c    0x20  w5500.o [1]
  .rodata            const    0x0800332c    0x20  w5500.o [1]
  .rodata            const    0x0800334c    0x20  weibo.o [1]
  .rodata            const    0x0800336c    0x20  weibo.o [1]
  .rodata            const    0x0800338c    0x20  weibo.o [1]
  .rodata            const    0x080033ac    0x20  weibo.o [1]
  .text              ro code  0x080033cc    0x20  printf.o [3]
  .text              ro code  0x080033ec    0x20  data_init2.o [4]
  .text              ro code  0x0800340c    0x1c  iarwstd.o [5]
  .text              ro code  0x08003428    0x1a  stm32f10x_it.o [1]
  .text              ro code  0x08003442    0x1a  zero_init2.o [4]
  .rodata            const    0x0800345c    0x18  w5500.o [1]
  .text              ro code  0x08003474    0x18  cmain.o [4]
  .text              ro code  0x0800348c    0x16  strchr.o [4]
  .text              ro code  0x080034a2    0x16  md5.o [1]
  .text              ro code  0x080034b8    0x16  xprout.o [3]
  .rodata            const    0x080034d0    0x14  device.o [1]
  .rodata            const    0x080034e4    0x14  device.o [1]
  .rodata            const    0x080034f8    0x14  device.o [1]
  .rodata            const    0x0800350c    0x14  main.o [1]
  .rodata            const    0x08003520    0x14  main.o [1]
  .rodata            const    0x08003534    0x14  socket.o [1]
  .text              ro code  0x08003548    0x14  exit.o [5]
  .rodata            const    0x0800355c    0x10  weibo.o [1]
  .rodata            const    0x0800356c    0x10  weibo.o [1]
  .text              ro code  0x0800357c    0x10  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800358c    0x10  util.o [1]
  .text              ro code  0x0800359c     0xe  div.o [3]
  .rodata            const    0x080035ac     0xc  weibo.o [1]
  .rodata            const    0x080035b8     0xc  weibo.o [1]
  .text              ro code  0x080035c4     0xa  cexit.o [4]
  .text              ro code  0x080035ce     0xa  xsprout.o [3]
  .rodata            const    0x080035d8     0x8  device.o [1]
  .rodata            const    0x080035e0     0x8  weibo.o [1]
  .rodata            const    0x080035e8     0x8  weibo.o [1]
  .rodata            const    0x080035f0     0x8  xprintffull.o [3]
  .text              ro code  0x080035f8     0x6  ABImemclr4.o [4]
  .text              ro code  0x080035fe     0x6  exit.o [3]
  .rodata            const    0x08003604     0x4  device.o [1]
  .rodata            const    0x08003608     0x4  device.o [1]
  .rodata            const    0x0800360c     0x4  device.o [1]
  .text              ro code  0x08003610     0x2  I64DivZer.o [4]
  .text              ro code  0x08003612     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003616     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800361a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800361e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003622     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003626     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800362a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800362e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003632     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003636     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800363a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800363e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003642     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003646     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800364a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800364e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003652     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003656     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800365a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800365e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003662     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003666     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800366a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800366e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003672     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003676     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800367a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800367e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003682     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003686     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800368a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800368e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003692     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003696     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800369a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800369e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036a2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036a6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036aa     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ae     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036b2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036b6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ba     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036be     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036c2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036c6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ca     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ce     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036d2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036d6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036da     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036de     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036e2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036e6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ea     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036ee     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036f2     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036f6     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036fa     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x080036fe     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003702     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003706     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800370a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800370e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003712     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003716     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800371a     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x0800371e     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003722     0x4  startup_stm32f10x_hd.o [1]
  .text              ro code  0x08003726     0x4  low_level_init.o [3]
  Initializer bytes  ro data  0x0800372c    0x2c  <for P2 s0>
                            - 0x08003758  0x3628

"P2", part 1 of 3:                         0x400
  CSTACK                      0x20000000   0x400  <Block>
    CSTACK           uninit   0x20000000   0x400  <Block tail>
                            - 0x20000400   0x400

"P2", part 2 of 3:                          0x2c
  P2 s0                       0x20000400    0x2c  <Init block>
    .data            inited   0x20000400    0x10  stm32f10x_rcc.o [1]
    .data            inited   0x20000410     0x8  device.o [1]
    .data            inited   0x20000418     0x8  device.o [1]
    .data            inited   0x20000420     0x4  stm32f10x_rcc.o [1]
    .data            inited   0x20000424     0x4  weibo.o [1]
    .data            inited   0x20000428     0x4  weibo.o [1]
                            - 0x2000042c    0x2c

"P2", part 3 of 3:                         0x228
  .bss               zero     0x2000042c   0x200  weibo.o [1]
  .bss               zero     0x2000062c    0x10  w5500.o [1]
  .bss               zero     0x2000063c    0x10  w5500.o [1]
  .bss               zero     0x2000064c     0x4  iarwstd.o [5]
  .bss               zero     0x20000650     0x2  socket.o [1]
                            - 0x20000652   0x226


*******************************************************************************
*** INIT TABLE
***

          Address     Size
          -------     ----
Zero (__iar_zero_init2)
    1 destination range, total size 0x226:
          0x2000042c  0x226

Copy (__iar_copy_init2)
    1 source range, total size 0x2c (100% of destination):
          0x0800372c   0x2c
    1 destination range, total size 0x2c:
          0x20000400   0x2c


*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
E:\WIZnet 产品文档\W5500\W5500\Application Reference\weibo_article\weibo\Debug\Obj: [1]
    SPI2.o                      180
    device.o                    336       96       16
    main.o                       72      108
    mcu_init.o                  440
    md5.o                        22
    misc.o                      160
    socket.o                    908       20        2
    startup_stm32f10x_hd.o      596
    stm32f10x_flash.o            60
    stm32f10x_gpio.o            348
    stm32f10x_it.o               26
    stm32f10x_rcc.o             832       20       20
    stm32f10x_spi.o             124
    stm32f10x_usart.o           394
    system_stm32f10x.o          344
    util.o                      140
    w5500.o                   1 408       88       32
    weibo.o                     304      400      520
    -------------------------------------------------
    Total:                    6 694      732      590

command line: [2]
    -------------------------------------------------
    Total:

dl7M_tl_in.a: [3]
    div.o                        14
    exit.o                        6
    low_level_init.o              4
    printf.o                     32
    sprintf.o                    48
    strstr.o                     48
    xdnorm.o                    198
    xdscale.o                   264
    xprintffull.o             3 266        8
    xprout.o                     22
    xsprout.o                    10
    -------------------------------------------------
    Total:                    3 912        8

rt7M_tl.a: [4]
    ABImemclr4.o                  6
    ABImemcpy.o                 112
    ABImemset.o                 102
    ABImemset48.o                56
    DblAdd.o                    230
    DblCmpGe.o                   46
    DblCmpLe.o                   46
    DblDiv.o                    582
    DblMul.o                    418
    DblSub.o                    382
    DblToI32.o                   86
    I32ToDbl.o                   46
    I64DivMod.o                 302
    I64DivZer.o                   2
    cexit.o                      10
    cmain.o                      24
    copy_init2.o                 36
    data_init2.o                 32
    memchr.o                     88
    strchr.o                     22
    strlen.o                     54
    zero_init2.o                 26
    -------------------------------------------------
    Total:                    2 708

shb_l.a: [5]
    exit.o                       20
    iarwstd.o                    28                 4
    -------------------------------------------------
    Total:                       48                 4

    Gaps                         22        6
    Linker created                        38    1 024
-----------------------------------------------------
    Grand Total:             13 384      784    1 618


*******************************************************************************
*** ENTRY LIST
***

Entry                      Address   Size  Type      Object
-----                      -------   ----  ----      ------
ADC1_2_IRQHandler       0x0800367f         Code  Wk  startup_stm32f10x_hd.o [1]
ADC3_IRQHandler         0x080036f3         Code  Wk  startup_stm32f10x_hd.o [1]
ADCPrescTable           0x20000420    0x4  Data  Lc  stm32f10x_rcc.o [1]
APBAHBPrescTable        0x20000400   0x10  Data  Lc  stm32f10x_rcc.o [1]
BusFault_Handler        0x0800342f    0x2  Code  Gb  stm32f10x_it.o [1]
CAN1_RX1_IRQHandler     0x0800368b         Code  Wk  startup_stm32f10x_hd.o [1]
CAN1_SCE_IRQHandler     0x0800368f         Code  Wk  startup_stm32f10x_hd.o [1]
CSTACK$$Base            0x20000000          --   Gb  - Linker created -
CSTACK$$Limit           0x20000400          --   Gb  - Linker created -
DMA1_Channel1_IRQHandler
                        0x08003663         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel2_IRQHandler
                        0x08003667         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel3_IRQHandler
                        0x0800366b         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel4_IRQHandler
                        0x0800366f         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel5_IRQHandler
                        0x08003673         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel6_IRQHandler
                        0x08003677         Code  Wk  startup_stm32f10x_hd.o [1]
DMA1_Channel7_IRQHandler
                        0x0800367b         Code  Wk  startup_stm32f10x_hd.o [1]
DMA2_Channel1_IRQHandler
                        0x08003717         Code  Wk  startup_stm32f10x_hd.o [1]
DMA2_Channel2_IRQHandler
                        0x0800371b         Code  Wk  startup_stm32f10x_hd.o [1]
DMA2_Channel3_IRQHandler
                        0x0800371f         Code  Wk  startup_stm32f10x_hd.o [1]
DMA2_Channel4_5_IRQHandler
                        0x08003723         Code  Wk  startup_stm32f10x_hd.o [1]
DebugMon_Handler        0x08003435    0x2  Code  Gb  stm32f10x_it.o [1]
Delay_ms                0x08002e9f   0x2e  Code  Gb  util.o [1]
Delay_us                0x08002e75   0x2a  Code  Gb  util.o [1]
EXTI0_IRQHandler        0x0800364f         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI15_10_IRQHandler    0x080036d7         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI1_IRQHandler        0x08003653         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI2_IRQHandler        0x08003657         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI3_IRQHandler        0x0800365b         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI4_IRQHandler        0x0800365f         Code  Wk  startup_stm32f10x_hd.o [1]
EXTI9_5_IRQHandler      0x08003693         Code  Wk  startup_stm32f10x_hd.o [1]
FLASH_IRQHandler        0x08003647         Code  Wk  startup_stm32f10x_hd.o [1]
FLASH_PrefetchBufferCmd
                        0x080030db   0x1c  Code  Gb  stm32f10x_flash.o [1]
FLASH_SetLatency        0x080030c1   0x1a  Code  Gb  stm32f10x_flash.o [1]
FSMC_IRQHandler         0x080036f7         Code  Wk  startup_stm32f10x_hd.o [1]
GPIO_Configuration      0x08001c89   0xb8  Code  Gb  mcu_init.o [1]
GPIO_Init               0x080022f1  0x150  Code  Gb  stm32f10x_gpio.o [1]
GPIO_ResetBits          0x08002447    0x6  Code  Gb  stm32f10x_gpio.o [1]
GPIO_SetBits            0x08002441    0x6  Code  Gb  stm32f10x_gpio.o [1]
HardFault_Handler       0x0800342b    0x2  Code  Gb  stm32f10x_it.o [1]
I2C1_ER_IRQHandler      0x080036b7         Code  Wk  startup_stm32f10x_hd.o [1]
I2C1_EV_IRQHandler      0x080036b3         Code  Wk  startup_stm32f10x_hd.o [1]
I2C2_ER_IRQHandler      0x080036bf         Code  Wk  startup_stm32f10x_hd.o [1]
I2C2_EV_IRQHandler      0x080036bb         Code  Wk  startup_stm32f10x_hd.o [1]
IINCHIP_CSoff           0x08000e01    0xa  Code  Gb  w5500.o [1]
IINCHIP_CSon            0x08000e0b    0xa  Code  Gb  w5500.o [1]
IINCHIP_READ            0x08000e5b   0x3a  Code  Gb  w5500.o [1]
IINCHIP_SpiSendData     0x08000e15    0xe  Code  Gb  w5500.o [1]
IINCHIP_WRITE           0x08000e23   0x38  Code  Gb  w5500.o [1]
MemManage_Handler       0x0800342d    0x2  Code  Gb  stm32f10x_it.o [1]
NMI_Handler             0x08003429    0x2  Code  Gb  stm32f10x_it.o [1]
NVIC_Configuration      0x08001dd1   0x70  Code  Gb  mcu_init.o [1]
NVIC_Init               0x08002cc7   0x6e  Code  Gb  misc.o [1]
NVIC_PriorityGroupConfig
                        0x08002cbd    0xa  Code  Gb  misc.o [1]
NVIC_SetVectorTable     0x08002d35    0xc  Code  Gb  misc.o [1]
PVD_IRQHandler          0x0800363b         Code  Wk  startup_stm32f10x_hd.o [1]
PendSV_Handler          0x08003437    0x2  Code  Gb  stm32f10x_it.o [1]
RCC_ADCCLKConfig        0x0800187d   0x16  Code  Gb  stm32f10x_rcc.o [1]
RCC_APB1PeriphClockCmd  0x08001995   0x1e  Code  Gb  stm32f10x_rcc.o [1]
RCC_APB2PeriphClockCmd  0x08001977   0x1e  Code  Gb  stm32f10x_rcc.o [1]
RCC_Configuration       0x08001d41   0x80  Code  Gb  mcu_init.o [1]
RCC_DeInit              0x08001701   0x5c  Code  Gb  stm32f10x_rcc.o [1]
RCC_GetClocksFreq       0x08001893   0xe4  Code  Gb  stm32f10x_rcc.o [1]
RCC_GetFlagStatus       0x080019b3   0x56  Code  Gb  stm32f10x_rcc.o [1]
RCC_GetSYSCLKSource     0x0800182f    0xa  Code  Gb  stm32f10x_rcc.o [1]
RCC_HCLKConfig          0x08001839   0x16  Code  Gb  stm32f10x_rcc.o [1]
RCC_HSEConfig           0x0800175d   0x4e  Code  Gb  stm32f10x_rcc.o [1]
RCC_IRQHandler          0x0800364b         Code  Wk  startup_stm32f10x_hd.o [1]
RCC_PCLK1Config         0x0800184f   0x16  Code  Gb  stm32f10x_rcc.o [1]
RCC_PCLK2Config         0x08001865   0x18  Code  Gb  stm32f10x_rcc.o [1]
RCC_PLLCmd              0x0800180d    0xa  Code  Gb  stm32f10x_rcc.o [1]
RCC_PLLConfig           0x080017ef   0x1e  Code  Gb  stm32f10x_rcc.o [1]
RCC_SYSCLKConfig        0x08001817   0x18  Code  Gb  stm32f10x_rcc.o [1]
RCC_WaitForHSEStartUp   0x080017ab   0x44  Code  Gb  stm32f10x_rcc.o [1]
RSIZE                   0x2000063c   0x10  Data  Lc  w5500.o [1]
RTCAlarm_IRQHandler     0x080036db         Code  Wk  startup_stm32f10x_hd.o [1]
RTC_IRQHandler          0x08003643         Code  Wk  startup_stm32f10x_hd.o [1]
Region$$Table$$Base     0x080032c8          --   Gb  - Linker created -
Region$$Table$$Limit    0x080032ec          --   Gb  - Linker created -
Reset_Handler           0x0800357d         Code  Wk  startup_stm32f10x_hd.o [1]
Reset_W5500             0x080025a5   0x26  Code  Gb  device.o [1]
SDIO_IRQHandler         0x080036fb         Code  Wk  startup_stm32f10x_hd.o [1]
SPI1_IRQHandler         0x080036c3         Code  Wk  startup_stm32f10x_hd.o [1]
SPI2_IRQHandler         0x080036c7         Code  Wk  startup_stm32f10x_hd.o [1]
SPI2_SendByte           0x08002c83   0x32  Code  Gb  SPI2.o [1]
SPI3_IRQHandler         0x08003703         Code  Wk  startup_stm32f10x_hd.o [1]
SPI_Cmd                 0x08002e39   0x1a  Code  Gb  stm32f10x_spi.o [1]
SPI_I2S_GetFlagStatus   0x08002e5b   0x1a  Code  Gb  stm32f10x_spi.o [1]
SPI_I2S_ReceiveData     0x08002e57    0x4  Code  Gb  stm32f10x_spi.o [1]
SPI_I2S_SendData        0x08002e53    0x4  Code  Gb  stm32f10x_spi.o [1]
SPI_Init                0x08002df9   0x40  Code  Gb  stm32f10x_spi.o [1]
SSIZE                   0x2000062c   0x10  Data  Lc  w5500.o [1]
SVC_Handler             0x08003433    0x2  Code  Gb  stm32f10x_it.o [1]
SetSysClock             0x0800249f    0x8  Code  Lc  system_stm32f10x.o [1]
SetSysClockTo72         0x080024a7   0xe0  Code  Lc  system_stm32f10x.o [1]
SysTick_Handler         0x08003439    0x2  Code  Gb  stm32f10x_it.o [1]
SystemInit              0x0800244d   0x52  Code  Gb  system_stm32f10x.o [1]
TAMPER_IRQHandler       0x0800363f         Code  Wk  startup_stm32f10x_hd.o [1]
TIM1_BRK_IRQHandler     0x08003697         Code  Wk  startup_stm32f10x_hd.o [1]
TIM1_CC_IRQHandler      0x080036a3         Code  Wk  startup_stm32f10x_hd.o [1]
TIM1_TRG_COM_IRQHandler
                        0x0800369f         Code  Wk  startup_stm32f10x_hd.o [1]
TIM1_UP_IRQHandler      0x0800369b         Code  Wk  startup_stm32f10x_hd.o [1]
TIM2_IRQHandler         0x0800343b    0x2  Code  Gb  stm32f10x_it.o [1]
TIM3_IRQHandler         0x0800343d    0x2  Code  Gb  stm32f10x_it.o [1]
TIM4_IRQHandler         0x080036af         Code  Wk  startup_stm32f10x_hd.o [1]
TIM5_IRQHandler         0x080036ff         Code  Wk  startup_stm32f10x_hd.o [1]
TIM6_IRQHandler         0x0800370f         Code  Wk  startup_stm32f10x_hd.o [1]
TIM7_IRQHandler         0x08003713         Code  Wk  startup_stm32f10x_hd.o [1]
TIM8_BRK_IRQHandler     0x080036e3         Code  Wk  startup_stm32f10x_hd.o [1]
TIM8_CC_IRQHandler      0x080036ef         Code  Wk  startup_stm32f10x_hd.o [1]
TIM8_TRG_COM_IRQHandler
                        0x080036eb         Code  Wk  startup_stm32f10x_hd.o [1]
TIM8_UP_IRQHandler      0x080036e7         Code  Wk  startup_stm32f10x_hd.o [1]
UART4_IRQHandler        0x08003707         Code  Wk  startup_stm32f10x_hd.o [1]
UART5_IRQHandler        0x0800370b         Code  Wk  startup_stm32f10x_hd.o [1]
USART1_IRQHandler       0x0800343f    0x2  Code  Gb  stm32f10x_it.o [1]
USART1_Init             0x080025cb   0x48  Code  Gb  device.o [1]
USART2_IRQHandler       0x08003441    0x2  Code  Gb  stm32f10x_it.o [1]
USART3_IRQHandler       0x080036d3         Code  Wk  startup_stm32f10x_hd.o [1]
USART_Cmd               0x080020cd   0x1a  Code  Gb  stm32f10x_usart.o [1]
USART_GetFlagStatus     0x0800214d   0x22  Code  Gb  stm32f10x_usart.o [1]
USART_ITConfig          0x080020e7   0x5e  Code  Gb  stm32f10x_usart.o [1]
USART_Init              0x08001fe5   0xe2  Code  Gb  stm32f10x_usart.o [1]
USART_SendData          0x08002145    0x8  Code  Gb  stm32f10x_usart.o [1]
USBWakeUp_IRQHandler    0x080036df         Code  Wk  startup_stm32f10x_hd.o [1]
USB_HP_CAN1_TX_IRQHandler
                        0x08003683         Code  Wk  startup_stm32f10x_hd.o [1]
USB_LP_CAN1_RX0_IRQHandler
                        0x08003687         Code  Wk  startup_stm32f10x_hd.o [1]
UsageFault_Handler      0x08003431    0x2  Code  Gb  stm32f10x_it.o [1]
WIZ_CS                  0x08002c5b   0x28  Code  Gb  SPI2.o [1]
WIZ_SPI_Init            0x08002c09   0x52  Code  Gb  SPI2.o [1]
WWDG_IRQHandler         0x08003637         Code  Wk  startup_stm32f10x_hd.o [1]
_GenldDefault           0x08000b59  0x24e  Code  Lc  xprintffull.o [3]
_LdtobDefault           0x08000745  0x40e  Code  Lc  xprintffull.o [3]
_LitobDefault           0x08000637  0x10e  Code  Lc  xprintffull.o [3]
_Printf                 0x08000131  0x506  Code  Gb  xprintffull.o [3]
_Prout                  0x080034b9   0x16  Code  Gb  xprout.o [3]
_PutcharsDefault        0x08000dc1   0x32  Code  Lc  xprintffull.o [3]
_SProut                 0x080035cf    0xa  Code  Gb  xsprout.o [3]
__aeabi_cdcmple         0x080031cd         Code  Gb  DblCmpLe.o [4]
__aeabi_cdrcmple        0x080031fd         Code  Gb  DblCmpGe.o [4]
__aeabi_d2iz            0x08003021         Code  Gb  DblToI32.o [4]
__aeabi_d2uiz           0x0800304d         Code  Gb  DblToI32.o [4]
__aeabi_dadd            0x08002a5d         Code  Gb  DblAdd.o [4]
__aeabi_ddiv            0x08001a41         Code  Gb  DblDiv.o [4]
__aeabi_dmul            0x08001e41         Code  Gb  DblMul.o [4]
__aeabi_dsub            0x08002171         Code  Gb  DblSub.o [4]
__aeabi_i2d             0x0800322d         Code  Gb  I32ToDbl.o [4]
__aeabi_ldiv0           0x08003611         Code  Gb  I64DivZer.o [4]
__aeabi_ldivmod         0x08002825         Code  Gb  I64DivMod.o [4]
__aeabi_memclr4         0x080035f9         Code  Gb  ABImemclr4.o [4]
__aeabi_memcpy          0x08002ef1         Code  Gb  ABImemcpy.o [4]
__aeabi_memcpy4         0x08002f0b         Code  Gb  ABImemcpy.o [4]
__aeabi_memcpy8         0x08002f0b         Code  Gb  ABImemcpy.o [4]
__aeabi_memset          0x08002f61         Code  Gb  ABImemset.o [4]
__aeabi_memset4         0x080030fd         Code  Gb  ABImemset48.o [4]
__aeabi_memset8         0x080030fd         Code  Gb  ABImemset48.o [4]
__aeabi_ui2d            0x08003241         Code  Gb  I32ToDbl.o [4]
__aeabi_uldivmod        0x08002839         Code  Gb  I64DivMod.o [4]
__exit                  0x08003549   0x14  Code  Gb  exit.o [5]
__iar_Dnorm             0x08002b43   0xc6  Code  Gb  xdnorm.o [3]
__iar_Dscale            0x08002955  0x108  Code  Gb  xdscale.o [3]
__iar_Memchr            0x08002fc9         Code  Gb  memchr.o [4]
__iar_Memset            0x08002f61         Code  Gb  ABImemset.o [4]
__iar_Memset4_word      0x08003105         Code  Gb  ABImemset48.o [4]
__iar_Memset8_word      0x08003105         Code  Gb  ABImemset48.o [4]
__iar_Memset_word       0x08002f69         Code  Gb  ABImemset.o [4]
__iar_Strchr            0x0800348d         Code  Gb  strchr.o [4]
__iar_Strstr            0x0800319d   0x30  Code  Gb  strstr.o [3]
__iar_copy_init2        0x080032a5   0x24  Code  Gb  copy_init2.o [4]
__iar_d2uiz             0x08003057         Code  Gb  DblToI32.o [4]
__iar_dadd              0x08002a6f         Code  Gb  DblAdd.o [4]
__iar_data_init2        0x080033ed   0x20  Code  Gb  data_init2.o [4]
__iar_dsub              0x08002183         Code  Gb  DblSub.o [4]
__iar_dsubStart         0x08002195         Code  Gb  DblSub.o [4]
__iar_program_start     0x08003475         Code  Gb  cmain.o [4]
__iar_sh_stdout_close   0x0800340d   0x16  Code  Gb  iarwstd.o [5]
__iar_sh_stdout_handle  0x2000064c    0x4  Data  Lc  iarwstd.o [5]
__iar_ui2d              0x08003243         Code  Gb  I32ToDbl.o [4]
__iar_zero_init2        0x08003443   0x1a  Code  Gb  zero_init2.o [4]
__low_level_init        0x08003727    0x4  Code  Gb  low_level_init.o [3]
__vector_table          0x08000000         Data  Gb  startup_stm32f10x_hd.o [1]
_exit                   0x080035c5         Code  Gb  cexit.o [4]
_main                   0x08003487         Code  Gb  cmain.o [4]
any_local_port          0x20000428    0x4  Data  Lc  weibo.o [1]
close                   0x0800145f   0x32  Code  Gb  socket.o [1]
connect                 0x08001491  0x108  Code  Gb  socket.o [1]
disconnect              0x08001599   0x24  Code  Gb  socket.o [1]
div                     0x0800359d    0xe  Code  Gb  div.o [3]
exit                    0x080035ff    0x6  Code  Gb  exit.o [3]
getGAR                  0x080010db   0x12  Code  Gb  w5500.o [1]
getIINCHIP_TxMAX        0x08000df5    0xc  Code  Gb  w5500.o [1]
getSIPR                 0x080010ff   0x12  Code  Gb  w5500.o [1]
getSUBR                 0x080010ed   0x12  Code  Gb  w5500.o [1]
getSn_IR                0x08001143   0x12  Code  Gb  w5500.o [1]
getSn_RX_RSR            0x080011d3   0x6c  Code  Gb  w5500.o [1]
getSn_SR                0x08001155   0x12  Code  Gb  w5500.o [1]
getSn_TX_FSR            0x08001167   0x6c  Code  Gb  w5500.o [1]
local_port              0x20000650    0x2  Data  Lc  socket.o [1]
main                    0x08003079   0x48  Code  Gb  main.o [1]
memchr                  0x08002fc9         Code  Gb  memchr.o [4]
memset                  0x080034a3   0x16  Code  Gb  md5.o [1]
post_weibo_update       0x080026f5  0x130  Code  Gb  weibo.o [1]
printf                  0x080033cd   0x20  Code  Gb  printf.o [3]
putchar                 0x08002ecd   0x20  Code  Gb  util.o [1]
recv                    0x080016b3   0x46  Code  Gb  socket.o [1]
recv_data_processing    0x080012cf   0x90  Code  Gb  w5500.o [1]
rxsize                  0x20000418    0x8  Data  Gb  device.o [1]
send                    0x080015bd   0xf6  Code  Gb  socket.o [1]
send_data_processing    0x0800123f   0x90  Code  Gb  w5500.o [1]
setGAR                  0x08001093   0x12  Code  Gb  w5500.o [1]
setRCR                  0x08001131   0x12  Code  Gb  w5500.o [1]
setRTR                  0x08001111   0x20  Code  Gb  w5500.o [1]
setSHAR                 0x080010b7   0x12  Code  Gb  w5500.o [1]
setSIPR                 0x080010c9   0x12  Code  Gb  w5500.o [1]
setSUBR                 0x080010a5   0x12  Code  Gb  w5500.o [1]
set_network             0x08002613   0xb4  Code  Gb  device.o [1]
socket                  0x08001375   0xea  Code  Gb  socket.o [1]
sprintf                 0x0800316d   0x30  Code  Gb  sprintf.o [3]
strchr                  0x0800348d         Code  Gb  strchr.o [4]
strlen                  0x08003135         Code  Gb  strlen.o [4]
strstr                  0x0800358d   0x10  Code  Gb  util.o [1]
sysinit                 0x08000f53  0x140  Code  Gb  w5500.o [1]
tmp_buf                 0x2000042c  0x200  Data  Gb  weibo.o [1]
txsize                  0x20000410    0x8  Data  Gb  device.o [1]
weibo_server_ip         0x20000424    0x4  Data  Gb  weibo.o [1]
wiz_read_buf            0x08000ef5   0x5e  Code  Gb  w5500.o [1]
wiz_write_buf           0x08000e95   0x60  Code  Gb  w5500.o [1]


[1] = E:\WIZnet 产品文档\W5500\W5500\Application Reference\weibo_article\weibo\Debug\Obj
[2] = command line
[3] = dl7M_tl_in.a
[4] = rt7M_tl.a
[5] = shb_l.a

  13 384 bytes of readonly  code memory
     784 bytes of readonly  data memory
   1 618 bytes of readwrite data memory

Errors: none
Warnings: none
